**Safe Work Practice**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Backfilling** | Development Date:**March 11th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Pain or injury from physical overexertion | Contact with machinery | Working in [extreme temperatures](http://www.ccohs.ca/oshanswers/phys_agents/hot_cold.html) and [UV radiation](http://www.ccohs.ca/oshanswers/phys_agents/ultravioletradiation.html). | Working with [hand tools](http://www.ccohs.ca/oshanswers/safety_haz/hand_tools/), [powered tools](http://www.ccohs.ca/oshanswers/safety_haz/power_tools/) and heavy powered equipment |
| Use of various machinery and tools. | Risk of eye injury from flying particles. |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Hearing Protection  | Eye Protection | Foot protection |  |
| High visibility reflective vests | Skin Protection  | Hearing Protection  |  |

**What are some good general safe work practices?**

* **DO NOT** backfill until all workers are clear of working areas.
* **DO** ensure the operators of any equipment being used in backfilling operations shall keep their spotters in sight at all times.
* **DO** ensure that Operators/Spotters are familiar with hand signals for their work site.
* **DO** ensure that all employees wear the appropriate PPE (including high visibility reflective vests).