**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Backfill from top of a bank** | Development Date:  **March 30th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Other workers & equipment | Working on lose ground | Machine malfunction |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Steel toed boots | Gloves | Hearing protection | Safety glasses |
| Hard hat | Safety vest |  |  |

**What is a proper safe job procedure to follow?**

* Designate a spotter who will be responsible for directing the driver/operator to the bank and to dump load
* Check ground for stability before proceeding to top of bank
* Ensure that all other workers are aware of and stay clear of the dump
* Follow through with dump when spotter signals it is safe to do so
* Once load is completely dumped, lower the box and carefully pull away from the bank