**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Band saw** | Development Date:  **March 30th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Exposed blades - cuts, amputations | Electrical shock | Excessive noise | Saw dust in eyes |
| Inhalation of saw dust particles |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Safety glasses | Dust mask | Steel toed boots | Hearing protection |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Ensure saw is unplugged or locked out
* Inspect work area to ensure clean
* Inspect electrical cords, switches, blade and guards for defects (all defective items will be tagged out of service)
* Inspect wood to ensure there are no defects or nails/screws in wood
* Place wood on work platform and measure height of wood
* Adjust guard to 1/8 inch above the height of wood
* Turn on saw and inspect blade as it runs to ensure no defects
* Push wood through saw and wait until blade stops to remove wood from platform
* Use a push stick if wood is small
* Unplug or lock
* If there is a lot of saw dust, wear a dust mask while cleaning