**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Bench or Floor Drill Press** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Gloves, loose clothing or jewelry being caught | Flying debris | Sparks  |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Face shield  | Safety glasses |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Read and understand instruction manual before operating drill press
* If you are not thoroughly familiar with the operation, obtain instruction from supervisor or other competent person.
* Do not operate while under the influence of medications, drugs or alcohol
* Always wear eye protection
* Guards and shield should be in place and used at all times
* Secure the material to be drilled securely with clamps or vise
* Adjust the speed of the drill as required
* Remove the chuck key form the chuck before starting the drill
* Make all adjustments with the power off
* Securely lock the drill bit into the chuck
* Shut off the power when you have completed drilling and remove the drill bit from the chuck
* Clean the table of debris before leaving the machine