**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Cold Start Equipment** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Equipment failure | Slips, trips & falls |  |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots |  |  |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Check all appropriate fluid levels and record in pre-trip book
* Visually inspect for leaks and worn belts
* Do a walk around inspection to ensure it is safe to start machine
* Proceed to start engine using the three point contact to enter machine
* Let machine idle and do another overall check for leaks
* Once machine is warm, proceed to task