**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Conveyor Cleaning/Maintenance** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Pinch points | Injury  | Amputation | Inhalation of dust particles |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Hand protection | Respiratory protection as required |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Do not wear loose or torn clothing
* Ensure all materials are off the belt
* Turn off the conveyor and lock it out
* Clean around the tail pulley, carrier and return rollers using a straight handled shovel (not “D” handle)
* Remove materials from underneath and around the conveyor
* Carry out maintenance/repairs as required
* Replace any guards or shields removed for cleaning and maintenance work
* Never jump or climb onto a conveyor for any reason while it is operating