**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Demolition** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Crushing  | Inhalation of hazardous materials | Lacerations  | Noise  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Eye protection | Hard hat | Steel toed boots | Respirator |
| Eye injuries | Hand protection | Safety vest |  |

**What is a proper safe job procedure to follow?**

* Do a thorough inspection of the site
* If possible, enter the building with supervisor to look for:
	+ People
	+ Appliances containing Freon
	+ Hazardous substance, such as asbestos and lead paint
	+ Tanks, wells, flammable or explosive material
* Ensure that all the proper permits have been obtained
* Ensure all utilities have been disconnected
* Notify property owner and adjoining property owners of time and date of demolition
* Demolitions to buildings adjoined to another building must be properly stabilized
* Barricade or fence the entire area to keep bystanders and traffic out of area
* Proceed with demolition
* Sort and haul away waste and rubble to appropriate facilities
* Clean up site as per local government regulations
* Remove barricades