**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Equipment Daily Maintenance** | Development Date:  **March 30th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Equipment failure | Collision | Pinch points |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Steel toed boots | Eye protection | Hand protection |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Walk around machine to check for tire damage, vandalism, any loose parts, or any other damage
* Check engine for:
  + Any frayed or damaged belts
  + Any damaged or leaking hoses
  + Engine mounting bolts are in place, tight and not damaged
* Check all fluid levels (some fluids may require the engine to be on, check manufacturers recommendations)
* Get into vehicle using 3 point contact method. Check for fire extinguisher and turn on engine
* Check all gauges:
  + Oil pressure is normal
  + Temperature is normal
  + Hydraulic pressure is normal (if gauge is applicable)
* Put machine in reverse to ensure back up alarm is working
* Do another walk around to check all lights
* Check brakes are working when pulling away to drive
* Proceed to job