**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Extinguishing & Dismantling Oxy Acetylene Equipment** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Burns | Inhalation of toxins | Fire and explosion hazard  |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Hand protection | Eye protection  |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Close Oxygen needle valve
* Close acetylene valve at torch end
* Close acetylene cylinder valve
* Close oxygen cylinder valve
* Drain acetylene by opening acetylene torch valve for a moment, then close again
* Drain oxygen in same manner as acetylene
* Re-open both torch valves
* Release pressure adjusting crews on both regulators
* Regulators and torches cannot be disconnected