**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Fuelling Vehicles** | Development Date:  **March 30th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Eye injury | Fire/Explosion | Skin exposure | Inhalation of hazardous vapors |
| Burns |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Steel toed boots | Eye protection | Hand protection |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Bring the vehicle to pump – ensure the side of the vehicle with tank access is closest to the pump
* Shut off ignition, extinguish any smoking material, leave cell phone in vehicle
* Remove fill cap
* Insert nozzle in to tank and flip pump lever to the “on” position
* Fill until desired quantity is obtained or until click is heard to indicate a full tank and then turn lever to the “off” position
* Place nozzle back on holder and replace the fill cap
* Wash any excess material off of hands promptly