**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Greasing a Vehicle** | Development Date:  **March 30th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Eye injury | Crush injuries | Burns | Potential death |
| Exposure to chemical |  |  |  |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Steel toed boots | Eye protection | Hand protection |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Shut off machine and utilize lock out procedure, including tagging and chocking the equipment
* Lay on creeper with grease gun, towel and roll under vehicle
* Clean each grease fitting and apply grease
* Check for fittings that need to be replaced
* Clean grease gun thoroughly when finished and put all tools used away
* Remove wheel chocks and lock out tags