**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Installation of Trench Box** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Asphyxiation | Loose grounding | Muscle strain | Fall injuries |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Steel toed boots | Eye protection | Hand protection | Hard hat |
| Visibility vest | Hearing protection |  |  |

**What is a proper safe job procedure to follow?**

* Assign a spotter who will be in charge of signaling operator and guiding trench box in trench
* Check grounding to ensure it is stable
* Ensure trench box is properly rigged to the machine by a competent rigger
* Begin the lift when all workers are at a safe distance and spotter signals to position over trench
* Slowly and cautiously lift trench box and follow direction of the spotter to position over trench
* Lower trench box as per spotter, be sure to keep trench box level
* Once trench box is in place wait for direction as to when it is clear to back away from the trench
* Back away slowly