**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Perimeter Fencing** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Vehicle or property damage | Serious injury | Vehicular and foot traffic |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Eye protection | Hand protection | Hard hat |
| Visibility vest |  |  |  |

**What is a proper safe job procedure to follow?**

* Inspect work area to determine the type and size of fencing to use (barricades, tape, snow fence, etc.)
* Take into consideration traffic control and work equipment travel patterns
* Erect perimeter fencing according to local regulations
* Proper signage is to be posted on fencing on each side of the fence
* The sign must include reasons for fencing, company name and contact number, name and contact number of supervisor
* Check fencing, at minimum, daily to ensure it hasn’t been removed or damaged
* Fencing and signage to be removed immediately upon completion of work