**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Supporting (Chocking) Dump Boxes** | Development Date:  **March 30th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Serious injury | Pinch points | Potential death |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Eye protection | Steel toed boots | Hand protection | Hard hat |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Park and block truck in neutral with the power take off (PTO) and pump engaged
* Raise truck box to desired level
* A Stiff Leg is a permanently attached pivot and rest, and is the preferred method of support
* If not available, use the following:
  + 6”x 6”x 6” long timber block across the truck frame between the box and subframe as close as possible to the box hinge
  + 2 pieces of 4”x 4”x 6” timber placed vertically between tandem tire and the box
  + Pin locks provided by the manufacturer to secure the box in the elevated position
* Only keep the box lifted for as long as required