**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Vehicle Daily Maintenance** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Equipment failure | Collision | Pinch points |  |
|  |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Eye protection | Hand protection |  |
|  |  |  |  |

**What is a proper safe job procedure to follow?**

* Walk around machine to check for damage, vandalism or any loose or worn parts.
* Check engine for:
	+ Any frayed or damaged belts
	+ Any damaged or leaking hoses
	+ Engine mounting bolts are in place, tight and not damaged
* Check all fluid levels (some fluids may require engine to be on, check manufacturers recommendations)
* Get into vehicle, using 3 point contact. Check for fire extinguisher and first aid kit.
* Turn on engine.
* Check all gauges. Ensure that:
	+ Oil pressure is normal
	+ Temperature is normal
	+ Hydraulic pressure is normal (if applicable)
* Put machine in reverse to ensure back up alarm is working
* Do another walk around to check all lights, get assistance if required
* Check brakes are working when pulling away to drive
* Proceed to job