**Safe Work Practice**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Opening And Guarding Manholes** | Development Date:  **February 24th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Slips, Trips, Falls | Environment | Cave -in | Contact with bacteria |
| Risk of eye injury from flying particles | [Extreme temperatures](http://www.ccohs.ca/oshanswers/phys_agents/hot_cold.html) when working outdoors. | . |  |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Head protection | Eye Protection | Foot protection | Hearing Protection |
| Respirator Equipment | Skin Protection |  |  |

**What are some good general safe work practices?**

* **DO** ensure obstructions to traffic shall be guarded by adequate signs, barricades, lights, flares or flags.
* **DO** ensure a blow torch or other open flame is not utilized to melt ice around a manhole or vault cover.
* **DO** ensure covers are removed and replaced by means of approved hooks or hoists.
* **DO** Ensue forced ventilation is used for oxygen deficiency.
* **DO** ensure equipment is in good working conditions.
* **DO** ensure you are trained in the use of breathing air apparatus.
* **DO** before any work is done on a cable, it shall be identified by an approved method.