**Safe Work Practice**

|  |  |  |
| --- | --- | --- |
| Name of Job:  **Use of a Roto Tiller & Edger** | Development Date:  **February 11th, 2011** | Developed By:  **CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Musculoskeletal injury (MSI) | Slips, trips & falls | Flying debris | Excessive noise |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Steel toed boots | Eye protection | Hand protection | Hearing protection |

**What are some good general safe work practices?**

* **DO** ensure all rocks and sharp objects are removed.
* **DO** ensure blades are on correctly.
* **DO** ensure hands, feet and hearing is protected.
* **DO NOT** service or fuel the equipment while it is running.
* **DO** follow safe job procedure for refueling as set out by the manufacture
* **DO** ensure the right mix of oil and gas is used.
* **DO** ensure head is greased.
* **DO** ensure guards are in place at all times.
* **DO** follow Roto Tiller and Edger manufacturer instructions for safe operation.