**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Confined Space Incident**  | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Claustrophobia | Injury or death | Asphyxiation | Potential acute or chronic health problems |
| Inhalation of fumes or vapors |  |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Eye protection | Hand protection | Fall arrest and quick retrieval equipment |
| Respiratory protection |  |  |  |

**What is a proper safe job procedure to follow?**

* Stop and clear all work in vicinity and ensure that no workers enter the confined space
* Utilize confined space rescue plan and call 911
* Secure the site against further danger or injuries
* Designate a worker to wait for emergency responders and lead them to accident area
* Hoist injured worker to surface
* Commence First Aid until relieved of responsibilities
* Begin accident investigation