**Safe Job Procedures**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Construction Laborers** | Development Date:**March 30th, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Slips, trips & falls  | Musculoskeletal injury (MSI) | Heavy machinery | Pinch points |
| Construction debris | Working alone |  | . |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
|  Steel toed boots | Eye protection | Hand protection | Hard hat |
| Reflective vest | Respiratory protection as required |  |  |

**What is a proper safe work procedure to follow?**

* Do an inspection of the work area before starting any task
* Make eye contact with all equipment operators to ensure they see you
* Stay alert and periodically look at surroundings to ensure safety
* Request assistance to move all heavy or awkward objects
* Practice good housekeeping
* If you identify a hazard – do what you can to fix it and report it to your supervisor for follow up
* Follow all the rules and Personal Protective Equipment requirements on the site