**Safe Work Practice**

|  |  |  |
| --- | --- | --- |
| Name of Job:**Pipeline tie-ins** | Development Date:**February 23rd, 2011** | Developed By:**CSNS** |

**Possible Hazards Present**

|  |  |  |  |
| --- | --- | --- | --- |
| Gas Release | Working in the sun  | Heavy machinery | Repetitive Tasks |
| Trench work |  |  |  |

**Personal Protective Equipment (PPE) and Devices Recommended**

|  |  |  |  |
| --- | --- | --- | --- |
| Head protection  | Eye Protection | Foot protection |  |
| Respirator Equipment | Skin Protection  | Hearing Protection  |  |

**What are some good general safe work practices?**

* DO regularly inspect equipment.
* DO remain within the operator’s line of vision.
* DO watch for moving equipment.
* DO Keep flammable materials away from areas where welding is being performed.
* DO ensure proper placement of skids.
* DO inspect slings before use.
* DO check field records for existing mains.
* DO be aware of pressure in the existing gas main.
* DO NOT ride on equipment unless appropriate seating is available.
* DO follow safe work procedures.