**Safe Work Practice Piling Installation**

| **Department/Area:** | **Approved by:** | **Date Created:** | **Review/Revision Date:** |
| --- | --- | --- | --- |
| insert text here |  |  |  |

| **Potential Hazard** | **Risk level** |
| --- | --- |
| Awkward/sustained postures - bend, reach, lift |  |
| Forceful exertions - lifting |  |
| Repetitive movements |  |
| Vibration |  |
| Compression |  |
| Sharp points/edges - sharp materials |  |
| Pinch points - bin lids |  |
| Materials falling - bin lids |  |
| Surfaces causing falls - icy, snow in winter |  |
| Moving machinery |  |
| Chemicals |  |
| Biological pathogens - contact with waste |  |
| Electrical |  |
| Extreme heat/cold |  |
| Noise |  |
| Combustibles/flammables |  |
| Risk of falling |  |
| Other |  |

| **Risk control devices, personal protective equipment, and other safety considerations** | **Training/Reference info** |
| --- | --- |
|  |  |

* DO set up signs and barricades.
* DO determine line locations and scope of locations.
* DO hand expose lines and cables.
* DO maintain minimum clearance from *underground*, overhead lines and structures.
* DO ensure awareness of pinch points.
* DO ensure tag lines are utilized.
* DO ensure proper isolation/ barricading/ covering/ of open excavations/ cages/ drive piles.
* DO ensure proper offloading of piling materials.
* DO ensure that auguring or drilling equipment is on stable ground and anchored properly.
* DO ensure you are visible at all times to the rig operator.
* DO follow piling safe work procedure step by step.