**Safe Work Practice Spray Painting**

| **Department/Area:** | **Approved by:** | **Date Created:** | **Review/Revision Date:** |
| --- | --- | --- | --- |
| insert text here |  |  |  |

| **Potential Hazard** | **Risk level** |
| --- | --- |
| Awkward/sustained postures - bend, reach, lift |  |
| Forceful exertions - lifting |  |
| Repetitive movements |  |
| Vibration |  |
| Compression |  |
| Sharp points/edges - sharp materials |  |
| Pinch points - bin lids |  |
| Materials falling - bin lids |  |
| Surfaces causing falls - icy, snow in winter |  |
| Moving machinery |  |
| Chemicals |  |
| Biological pathogens - contact with waste |  |
| Electrical |  |
| Extreme heat/cold |  |
| Noise |  |
| Combustibles/flammables |  |
| Risk of falling |  |
| Other |  |

| **Risk control devices, personal protective equipment, and other safety considerations** | **Training/Reference info** |
| --- | --- |
|  |  |

**What are some general safe work practices**?

* **DO** Ensure you are fully trained.
* **DO** Follow manufacturer’s recommendations on safe use and recommended personal protective equipment (PPE)
* **DO** ensure all sources of ignition are eliminated or controlled.
* **DO** ensure equipment is grounded.
* **DO** ensure area is well ventilated.
* **DO** NOT smoke around spray painting operations.
* **DO** ensure warning signs are in place.
* **DO** Use proper PPE when spray painting such as self contained breathing apparatus (SCBA) or respirator depending on the task and process
* **DO** Always wash hands prior to smoking or eating