Chemical Storage

* chemicals should be stored no higher than eye level and
* never on the top shelf of a storage unit.
* Do not overcrowd shelves.
* Each shelf should have an anti-roll lip.
* Avoid storing chemicals on the floor (even temporarily) or extending into traffic aisles.
* Store in a corrosive's cabinet, if available, or in compatible secondary containment.
* Bases should be segregated from acids, flammables, and reactive.
* Call the manufacturer directly for storage requirements and refer to applicable regulations.